|  |  |
| --- | --- |
| **VHF EXPOSED DIPOLES** | **138-174 MHz** |

**Logo

Description automatically generatedF-33030-D**


The F-33030-D is a Wide Band Omnidirectional Antenna specifically designed for trunked multicoupled and X-pass systems applications. This antenna is extremely rugged and is well suited for use in severe environmental conditions. This antenna is a Low Intermod design that incorporates a minimum of moveable joints in its construction and replaces standard castings with heavy duty welded joints.


* The F-33030-D has internal cabling design and is not field adjustable.
* Passive Intermodulation Specification is measured in the third order intermodulation products, using two 25 watts (+44 dBm) Carriers.

|  |  |
| --- | --- |
| **Electrical Specifications** | **F-33030-D** |
| Frequency Range, MHz | 138-174 |
| Nominal Gain, dBd | 6 |
| Number of Dipoles | 8 |
| Bandwidth 1.5:1 VSWR, MHz | 36 |
| Polarization | Vertical |
| Pattern | Omni |
| Power Rating, Watts | 500 |
| Nominal Impedance, Ohms | 50 |
| Lightning Protection | DC Ground |
| Passive Intermodulation | -107 dBm (-150 dBc) |
| Standard Termination | 7/16 DIN male connector attached to end of 118 in (3000 mm) RG-214 Cable |
| **Mechanical Specifications** | **F-33030-D** |
| Length, in (mm) | 246 (6248) |
| Width (1/2 Wave Spacing), in (mm) | 30 (762) |
| Weight, lbs. (kg) | 130 (59) |
| Lateral Thrust lb (N) | 297 (1319) |
| Bending moment at top clamp lb-ft (N-m) | 2107 (2857) |
| Wind Zone | 1000 Pa |
| Material | Aluminum 6061-T6 |
| Projected Area, ft² (m²) | 11,1 (1,03) |
| Mounting Information Mast O.D. (mm) | Mast 4,5" (114.3 mm) O.D. |



|  |  |
| --- | --- |
| **VHF EXPOSED DIPOLE** | **138-174 MHz** |





Horizontal (Azimuth) Radiation Pattern

Vertical (Elevation) Radiation Pattern